365 ALUTEC ROOF OUTLETS  
  
 Manufacturer: Marley Alutec, Unit 1 (G-H), Hudson Road,  
 Elms Farm Industrial Estate, Bedford MK41 0LZ  
 Tel: 01234 359438, Fax: 01234 357199.  
 Email: enquiries@marleyalutec.co.uk  
 Reference: Alutec Elite aluminium roof/car park outlet  
 Type: Vertical threaded connector – 500mm length  
 Product code: AR110F

Connection size: 110mm OD

Grate Type: Flat grate (1.5 tonne load rating)

Waterproofing type: Suitable for use with all types (Liquid, single ply, hotmelt, GRP, bituminous etc)

Flow Performance: 10.7 litres per second

Type / grade: Marine grade Aluminium alloy to BSEN1559:1997,   
 BSEN 1676:1997 and BSEN 1706:1998

Functional life expectancy: 50 years