311 TRADITIONAL ALUMINIUM GUTTERS

 Manufacturer: Marley Alutec, Unit 1 (G-H), Hudson Road,
 Elms Farm Industrial Estate, Bedford MK41 0LZ
 Tel: 01234 359438, Fax: 01234 357199.
 Email: enquiries@marleyalutec.co.uk
 Gutters and fittings to: BS 8530

Reference: Traditional Victorian Ogee aluminium rainwater system
 Profile: Victorian Ogee
 Size: 125mm
 Outlet Size: 63mmØ, 76mmØ, 72x72 mm or 102x76mm (selected by spec builder drop down)
 Type / grade: Marine grade Aluminium alloy to BSEN1559:1997,
 BSEN 1676:1997 and BSEN 1706:1998
Finish: Polyester powder coated to BS EN 12206-1:2004
 Colour: (selected by spec builder drop down)
 Functional life expectancy: 50 years

Jointing: Gutter lengths or fittings are overlapped at the joint with a spigot and socket. Slots are provided for fixing using Alutec M6 aluminium bolts with nuts and washers. Seal evenly across the joints with Alutec sealant
Fixing: Fascia bracket fixed at 915mm centres and at each fitting using Alutec 32mm x No. 10 round head austenitic stainless steel screws